Firmware Version: v26.5.44R
Release Date: June 15th, 2026
---------------------------------------------
Update Monitor: SWIT BM-H245
---------------------------------------------

What's New:

[20260615 v26.5.44R]
1. Add - TimeCode Text color, brightness, transparency adjustment
2. Add - Multiview functions assigned to Function Keys
3. False color display effect optimized
4. Fixed incorrect parsing of the payload ID
5. Fixed an issue where rapid repeated hot-plugging of the video cable in Quad-view mode could occasionally cause the image to freeze on the last frame.
6. Improved HDMI signal compatibility with Canon cameras.

[20260113 v24.5.42R]
1. Add JETI SPECBOS 2501 support for Auto calibration
2. Fixed system freeze issue after Auto Calibration by X-rite i1 Probe
3. Add User-log selection in Delog Menu

[20240628 v21.5.38R]
1. Add new function: Anamorphic De-squeeze 
2. Add Input source selection in F1-F5 keys
3. Add new input range selection: 64-1023
4. Optimized the adjust precision of RGB GAIN/BIAS and CBS
5. Optimized the PBP H/V setting menu
6. Optimized the default display position of the overlay charts
7. Optimized the default transparent of waveforms

[20240318 v20.5.37R]
1. Fixed the issue of 2 pixels missed in left and right edge  
2. Fixed the bug of surround sound pattern lost when returning from PIP mode.
3. Fixed the error of CIE pattern in some video formats.
4. Set the default color gamut as Rec.709 instead of LCD Native.
5. Add vertical crop display in PBP mode


---------------------------------------------

Update Steps:

★★★★★  IMPORTANT NOTE  ★★★★★
Please check your current firmware version and select a correct firmware to update.
→ Current firmware version before v4.5.31R:
    Please use BM-H245_v26.5.44R_before4.5.31R_20260615_1656.zip
→ Current firmware version is v4.5.31R or later than v4.5.31R:
    Please use BM-H245_v26.5.44R_20260612_0942.zip

1. Copy the firmware file correct firmware pack file according to your current version to USB disk (FAT32 file format), root directory. Do not unzip. Make sure there's no other firmware pack file start with "BM-H245" in the root directory of the USB disk.
2. Plug the USB disk into front USB port of the monitor.
3. Enter Menu - System - Update - YES, the monitor will update and follow the on-screen instruction to restart. DO NOT power off the monitor during updating.
4. After monitor restarted, plug off the USB disk
5. Enter Menu - Exit & Status, check firmware version should be v26.5.44R.
(Finish)

---------------------------------------------
